{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["FLWMTF","Flex Face Dimensions"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":23,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"FLWMTF","index":0,"n_rows":40,"n_cols":36,"rows_kept":40,"cut":false,"hidden":false,"merged":[[39,35,39,36],[35,1,35,28],[36,1,36,28],[37,1,37,28],[38,2,38,3],[38,4,38,28],[13,1,13,28],[39,2,39,3],[39,4,39,25],[18,1,18,28],[19,1,19,28],[8,1,8,25],[10,1,10,28],[3,1,3,28],[6,28,8,28],[6,26,8,26],[6,27,8,27],[9,1,9,28],[4,1,5,28],[1,1,1,28],[14,5,14,6],[14,7,14,28],[6,18,6,25],[7,1,7,4],[2,1,2,28],[6,1,6,4],[6,5,6,13],[7,17,7,18],[14,2,14,3],[7,5,7,6],[6,14,6,17],[7,11,7,12],[7,7,7,10],[7,13,7,16],[7,19,7,25],[11,31,11,32],[18,31,18,32],[30,1,30,28],[23,1,23,28],[24,1,24,28],[25,1,25,28],[26,1,26,28],[28,2,28,3],[27,1,27,28],[28,4,28,28],[11,1,12,28],[15,7,15,25],[16,2,16,3],[16,5,16,6],[15,2,15,3],[15,5,15,6],[4,30,4,32],[4,33,4,34],[31,1,31,28],[21,2,21,3],[20,5,20,6],[21,5,21,6],[21,7,21,25],[20,2,20,3],[22,5,22,6],[22,7,22,25],[22,2,22,3],[20,7,20,28],[29,2,29,3],[29,4,29,25],[17,1,17,28],[16,7,16,25],[34,35,34,36],[32,1,32,28],[33,2,33,3],[34,2,34,3],[33,4,33,28],[34,4,34,25]]}
[]
[]
[]
[null,"BILL OF MATERIALS"]
[null,{"$f":"IF(KQ=0,\"\",AE5&AJ5&AH5)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(BOD=1,\"\",IF(BodyType=1,\" Front Load Wall Mount Tension Frame\",\"\"))","v":" Front Load Wall Mount Tension Frame"},null,null,{"$f":"IF(BodyType=5,\"\",IF(FRMRET=1,\" Front Load Wall Mount Tension Frame Cover\",\"\"))","v":" Front Load Wall Mount Tension Frame Cover"},null,{"$f":"IF(BOD=1,\"\",IF(BodyType=1,\" with\",IF(BodyType=2,\" with\",IF(BodyType=3,\" with\",IF(BodyType=4,\" with\",IF(BodyType=5,\"\",\"\"))))))","v":" with"}]
[]
[null,"Customer  ",null,null,null,null,null,null,null,null,null,null,null,null,"Order#   ",null,null,null,null,null,null,null,null,null,null,null,"Lengths Required","Lengths Used","Drops Used"]
[null,"Kit Quantity  ",null,null,null,0,null,"Height  ",null,null,null,0,null,"Width",null,null,null,0]
[]
[null,"Extrusions"]
[]
[null,"Body Type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Body Type",null,2,"Body"]
[]
[]
[null,"Qty.","Size (in)",null,"x","Part #",null,"  Description"]
[null,{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(AND(BodyType>=1,BodyType<=4),KQ*2,\"\")))","v":""},{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(BodyType=1,Wdt,\"\")))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(BodyType=1,\"2080\",\"\")))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(BodyType=1,\" Front Load Wall Mount Tension Frame - Top & Bottom - Mitered both Ends\",\"\")))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(AND(BodyType>=1,BodyType<=4),KQ*2,\"\")))","v":""},{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(BodyType=1,Hgt,\"\")))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(BodyType=1,\"2080\",\"\")))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(BodyType=1,\" Front Load Wall Mount Tension Frame - Ends - Mitered Both Ends\",\"\")))","v":""}]
[]
[null,"Cover",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Frame Retainer",null,2,"Ret"]
[]
[null,"Qty.","Size (in)",null,"x","Part #",null,"  Description"]
[null,{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(OR(OR(BodyType=1,BodyType=4,BodyType=5)),KQ*2,IF(OR(BodyType=2,BodyType=3),KQ*4,\"\"))))","v":""},{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(BodyType=1,Wdt,\"\")))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(FRMRET=1,\"2078\",\"\")))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(FRMRET=1,\" Front Load Wall Mount Tension Frame Cover- Top and Bottom - Mitered Both Ends\",\"\")))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(OR(OR(BodyType=1,BodyType=4,BodyType=5)),KQ*2,IF(OR(BodyType=2,BodyType=3),KQ*4,\"\"))))","v":""},{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(BodyType=1,Hgt,\"\")))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(FRMRET=1,\"2078\",\"\")))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(FRMRET=1,\" Front Load Wall Mount Tension Frame Cover- Sides - Mitered Both Ends\",\"\")))","v":""}]
[]
[null,"Hardware"]
[]
[null,"Body"]
[]
[null,"Qty.","Part #",null,"Description"]
[null,{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(BodyType=1,KQ*4,\"\")))","v":""},{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(BodyType=1,\"5323\",\"\")))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(BOD=1,\"\",IF(BodyType=1,\" Front Load Wall Mount Tension Frame Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (1-1/2'') - One (1) per corner\",\"\")))","v":""}]
[]
[null,"Frame Retainer"]
[]
[null,"Qty.","Part #",null,"Description"]
[null,{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(BodyType=1,(MMH+2)*KQ,\"\")))","v":""},{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(FRMRET=1,\"5195\",\"\")))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(RET=1,\"\",IF(FRMRET=1,\" Cover Screw - #8 x 5/16'' steel zinc sq/phillps pan head screw- Every 18'' on Center along outside perimeter\",\"\")))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ROUNDUP((Hgt/18)+1,0)","v":1},{"$f":"ROUNDUP((Wdt/18)+1,0)","v":1},{"$f":"ROUNDUP((Hgt/18)+1,0)","v":1},{"$f":"ROUNDUP((Wdt/18)+1,0)","v":1},{"$f":"SUM(AE35:AH35)","v":4},"Cover Screws"]
[]
[null,"Tension Clips"]
[]
[null,"Qty.","Part #",null,"Description"]
[null,{"$f":"IF(KQ=0,\"\",IF(BodyType=1,TTC*KQ,\"\"))","v":""},{"$f":"IF(KQ=0,\"\",IF(FRMRET=1,\"5360\",\"\"))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(FRMRET=1,\" Tension Clip - One (1) every 6'' on center\",\"\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ROUNDUP((Hgt/6)+2,0)","v":2},{"$f":"ROUNDUP((Wdt/6)+2,0)","v":2},{"$f":"ROUNDUP((Hgt/6)+2,0)","v":2},{"$f":"ROUNDUP((Wdt/6)+2,0)","v":2},{"$f":"SUM(AE40:AH40)","v":8},"Tension Clips"]

{"sheet":"Flex Face Dimensions","index":1,"n_rows":58,"n_cols":31,"rows_kept":58,"cut":false,"hidden":false,"merged":[[1,1,1,28],[2,1,2,28],[3,1,3,28],[4,1,5,28],[6,1,6,28],[7,1,7,28],[8,1,8,28],[25,1,25,28],[26,1,26,4],[26,5,26,21],[26,22,26,28],[27,1,27,28],[28,3,28,9],[28,10,28,11],[28,13,28,19],[28,20,28,21],[28,22,28,28],[29,1,29,28],[30,3,30,9],[30,10,30,11],[30,13,30,19],[30,20,30,21],[30,22,30,28],[31,1,31,28],[32,3,32,9],[32,10,32,11],[32,13,32,19],[32,20,32,21],[32,22,32,28],[33,1,33,28],[34,1,34,28],[35,1,35,28],[52,1,52,28],[53,8,53,12],[53,13,53,14],[53,15,53,24],[54,1,54,28],[55,7,55,12],[55,13,55,14],[55,15,55,24],[57,7,57,12],[57,13,57,14],[57,15,57,26]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Face Trim Size Calculations"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Frame Type:",null,null,null,{"$f":"IF(KQ=0,\"\",IF(AND(BodyType=1,FRMRET=1),\" 6'' Flat Bleed Single Face Tension Body and Cover\",\"\"))","v":""}]
[]
[null,null,null,"Outside Frame dimension (Height) ",null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",Hgt)","v":""},null,null,"Outside Frame Dimension (Width) ",null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",Wdt)","v":""}]
[]
[null,null,null,"Visual Opening (Height) ",null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(AND(BodyType=1,FRMRET=1),Hgt-2.75,\"\"))","v":""},null,null,"Visual Opening (Width) ",null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(AND(BodyType=1,FRMRET=1),Wdt-2.75,\"\"))","v":""}]
[]
[null,null,null,"Face Trim Size (Height) ",null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(AND(BodyType=1,FRMRET=1),OFDH+4.5,\"\"))","v":""},null,null,"Face Trim Size (Width) ",null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(AND(BodyType=1,FRMRET=1),OFDW+4.5,\"\"))","v":""}]
[]
[]
[null,"Clip Line Calculations"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Clip Line Placement ",null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(BodyType=1,\"1-1/2''\",\"\"))","v":""},null,"(In from the trimmed edge of the face.)"]
[]
[null,null,null,null,null,null,null,"Clip Spacing ",null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(BodyType=1,\"6''\",\"\"))","v":""},null,"(Center to Center)"]
[]
[null,null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(BodyType=1,\"Tensioning Tool \",\"\"))","v":""},null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(BodyType=1,\"5137\",\"\"))","v":""},null,"(See Product Guide Pg. 12 or Contact Customer Service)"]