{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Standard","Gas Support","GS Placement A","GS Placement B","GS Placement C"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":2,"defined_names":88,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Standard","index":0,"n_rows":116,"n_cols":36,"rows_kept":116,"cut":false,"hidden":false,"merged":[[110,1,110,28],[112,2,112,3],[113,2,113,3],[114,2,114,3],[115,2,115,3],[112,6,112,7],[113,6,113,7],[114,6,114,7],[115,6,115,7],[112,10,112,11],[113,10,113,11],[114,10,114,11],[115,10,115,11],[112,14,112,15],[113,14,113,15],[114,14,114,15],[115,14,115,15],[112,18,112,19],[113,18,113,19],[114,18,114,19],[115,18,115,19],[96,35,96,36],[90,31,90,33],[86,30,86,40],[56,33,56,35],[56,30,56,32],[53,31,53,32],[48,31,48,32],[46,31,46,32],[109,4,109,25],[83,4,83,25],[77,4,77,25],[79,4,79,25],[71,5,71,6],[75,28,77,28],[80,4,80,25],[81,4,81,25],[71,7,71,10],[71,11,71,12],[71,13,71,16],[57,5,57,6],[56,5,56,6],[51,5,51,6],[57,7,57,25],[56,7,56,25],[109,2,109,3],[108,28,109,28],[88,2,88,3],[57,2,57,3],[86,28,91,28],[87,2,87,3],[58,1,58,28],[59,5,59,6],[59,7,59,25],[74,1,74,28],[59,2,59,3],[78,1,78,28],[79,2,79,3],[80,2,80,3],[81,2,81,3],[79,28,84,28],[68,1,68,28],[70,1,70,4],[107,1,107,28],[108,2,108,3],[108,4,108,25],[67,1,67,28],[84,4,84,25],[83,2,83,3],[84,2,84,3],[102,4,102,25],[103,2,103,3],[103,4,103,25],[92,1,92,28],[93,2,93,3],[93,4,93,25],[94,2,94,3],[94,4,94,25],[100,4,100,25],[100,2,100,3],[104,2,104,3],[104,4,104,25],[98,28,104,28],[64,1,64,28],[66,1,66,28],[69,1,69,28],[77,2,77,3],[89,2,89,3],[90,2,90,3],[91,2,91,3],[87,4,87,25],[88,4,88,25],[89,4,89,25],[90,4,90,25],[91,4,91,25],[70,14,70,17],[70,18,70,25],[65,1,65,28],[96,4,96,25],[101,2,101,3],[101,4,101,25],[86,2,86,3],[86,4,86,25],[96,2,96,3],[51,7,51,25],[51,2,51,3],[53,1,54,28],[55,1,55,28],[56,2,56,3],[71,17,71,18],[71,19,71,28],[71,1,71,4],[72,1,72,28],[70,5,70,13],[70,26,70,28],[82,2,82,3],[82,4,82,25],[1,1,1,28],[18,5,18,6],[18,7,18,28],[8,18,8,25],[9,1,9,4],[5,1,5,28],[6,1,6,28],[3,1,3,28],[8,1,8,4],[8,5,8,13],[10,1,10,18],[9,17,9,18],[9,19,10,25],[18,2,18,3],[9,5,9,6],[8,14,8,17],[9,11,9,12],[4,1,4,28],[8,28,10,28],[12,1,12,28],[2,1,2,28],[50,7,50,25],[106,2,106,3],[106,4,106,25],[99,2,99,3],[99,4,99,25],[52,1,52,28],[25,5,25,6],[26,5,26,6],[25,2,25,3],[26,2,26,3],[76,2,76,3],[73,1,73,28],[75,2,75,3],[97,1,97,28],[98,2,98,3],[98,4,98,25],[76,4,76,25],[93,28,96,28],[95,2,95,3],[95,4,95,25],[105,1,105,28],[75,4,75,25],[85,1,85,28],[102,2,102,3],[63,1,63,28],[50,2,50,3],[50,5,50,6],[20,5,20,6],[19,2,19,3],[19,5,19,6],[49,1,49,28],[48,1,48,28],[27,1,27,28],[28,1,28,28],[29,1,29,28],[40,23,40,28],[41,1,41,28],[42,2,42,3],[34,2,34,3],[44,2,44,3],[42,5,42,6],[44,5,44,6],[44,7,44,25],[42,7,42,28],[43,2,43,3],[43,5,43,6],[15,32,15,33],[8,30,8,33],[9,30,9,33],[25,7,25,25],[9,7,9,10],[9,13,9,16],[21,1,21,28],[24,7,24,28],[40,15,40,22],[40,1,40,3],[26,7,26,25],[24,2,24,3],[28,31,28,32],[19,7,19,25],[20,2,20,3],[43,30,43,33],[17,1,17,28],[24,5,24,6],[23,1,23,28],[22,1,22,28],[5,34,5,37],[30,1,30,28],[31,2,31,3],[32,2,32,3],[31,5,31,6],[32,5,32,6],[32,7,32,25],[5,30,5,33],[6,30,6,33],[8,26,10,26],[8,27,10,27],[11,1,11,28],[16,1,16,28],[13,1,15,28],[7,1,7,28],[10,30,10,36],[13,31,13,32],[20,7,20,25],[31,7,31,28],[106,30,106,34],[107,30,107,34],[108,30,108,34],[6,34,6,37],[25,30,25,32],[3,30,3,31],[34,5,34,6],[34,7,34,25],[35,2,35,3],[47,1,47,28],[36,1,36,28],[37,1,37,28],[46,1,46,28],[40,5,40,12],[29,31,29,32],[45,1,45,28],[43,7,43,25],[35,7,35,25],[33,2,33,3],[33,5,33,6],[33,7,33,25],[38,1,38,28],[39,1,39,28],[35,5,35,6]]}
[]
[]
[]
[null,"BILL OF MATERIALS",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(Body<=3,\" 1Part 2Part\",IF(Body=4,\" 2Part\",IF(Body=5,\" Retro Fit -\"))))","v":""}]
[]
[null,{"$f":"IF(KQ=0,\"\",AI6&AE4&AE6&AE7&AE9&AE10&AI7)","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(BodyType=1,\" 6'' Single Face Body\",IF(BodyType=2,\" 8'' Single Face Body\",IF(BodyType=3,\" 6'' Double Face Body\",IF(BodyType=4,\" 9'' Double Face Body\",IF(BodyType=5,\" 12'' Double Face Body\")))))))","v":""},null,null,null,{"$f":"IF(PTDS=1,\"Mill Finish -\",IF(PTDS=2,\"Pre-Painted -\"))","v":"Mill Finish -"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(NOYES=2,\"\",IF(Body=1,\" with One End Removable\",IF(Body=2,\" with Both Ends Removable\",IF(Body=3,\" All Sides\",(IF(AND(Body=4,RETTYPE=1),\" with 2Part Retainer\",(IF(AND(Body=4,RETTYPE=2),\" with 2Part Extended Retainer\",(IF(AND(Body=4,RETTYPE=3),\" with 2Part Extended Retainer - One End Removable\",(IF(AND(Body=4,RETTYPE=4),\" with 2Part Extended Retainer - Both Ends Removable\",(IF(AND(Body=4,RETTYPE=5),\" with 2Part Large Extended Retainer\",\"\"))))))))))))))","v":" with One End Removable"},null,null,null,{"$f":"IF(NOYES=2,\"\",(IF(AND(Body=5,RETTYPE=1),\" 2Part Retainer\",(IF(AND(Body=5,RETTYPE=2),\" 2Part Extended Retainer\",(IF(AND(Body=5,RETTYPE=3),\" 2Part Extended Retainer - One End Removable\",(IF(AND(Body=5,RETTYPE=4),\" 2Part Extended Retainer - Both Ends Removable\",(IF(AND(Body=5,RETTYPE=5),\" 2Part Large Extended Retainer\",\"\")))))))))))","v":""}]
[]
[null,"Customer  ",null,null,null,null,null,null,null,null,null,null,null,null,"Order#   ",null,null,null,null,null,null,null,null,null,null,null,"Lengths Required","Lengths Used","Drops Used",null,{"$f":"IF(NOYES=1,\"\",IF(AND(Body=4,INFRM=1),\" with Vandal Cover\",IF(AND(Body=4,INFRM=2),\" with Large Vandal Cover\",IF(AND(Body=5,INFRM=1),\" Vandal Cover\",IF(AND(Body=5,INFRM=2),\" Large Vandal Cover\",\"\")))))","v":""}]
[null,"Kit Quantity  ",null,null,null,0,null,"Height  ",null,null,null,0,null,"Width",null,null,null,0,null,{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(OR(BodyType<=2,BodyType>=4),\"Add 1-3/4'' to the overall height or width in the direction the lamps will be placed.\",IF(BodyType=3,\"Add 1'' to the overall height or width in the direction the lamps will be placed.\",\"\"))))","v":""},null,null,null,null,null,null,null,null,null,null,{"$f":"IF(NOYES=2,\"\",(IF(AND(NoYes2=2,RETTYPE=1),\" and 2Part Divider\",(IF(AND(NoYes2=2,RETTYPE=2),\" with 2Part Divider\",(IF(AND(NoYes2=2,RETTYPE=3),\" with 2Part Divider\",(IF(AND(NoYes2=2,RETTYPE=4),\" with 2Part Divider\",(IF(AND(NoYes2=2,RETTYPE=5),\" and 2Part Divider\",\"\")))))))))))","v":""}]
[null,"Enter Fractions as Decimals",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Add 1'' to the overall height or width in the direction the lamps will be placed."]
[null,"Extrusions"]
[]
[null,"Body Type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Body Type"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Body"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,{"$f":"IF(PTDS=1,\"\",IF(PTDS=2,\"P\"))","v":""},"Mill or Painted"]
[null,"1Part Body"]
[]
[null,"Qty.","Size (in)",null,"x","Part #",null,"  Description"]
[null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=4,\"\",IF(Body=5,\"\",IF(AND(BodyType<=5,Body<=3),KQ*2,\"\")))))","v":""},{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=4,\"\",IF(Body=5,\"\",IF(AND(BodyType<=5,Body<=3),Wdt,\"\")))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=4,\"\",IF(Body=5,\"\",IF(BodyType=1,\"1921\"&PPTD,IF(BodyType=2,\"1922\"&PPTD,IF(BodyType=3,\"1931\"&PPTD,IF(BodyType=4,\"1923\"&PPTD,IF(BodyType=5,\"1924\"&PPTD,\"\")))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=4,\"\",IF(Body=5,\"\",IF(BodyType=1,\" 1Part 6'' Single Face Body - Top & Bottom - Mitered both ends\",IF(BodyType=2,\" 1Part 8'' Single Face Body - Top & Bottom - Mitered both ends\",IF(BodyType=3,\" 1Part 6'' Double Face Body - Top & Bottom - Mitered both ends\",IF(BodyType=4,\" 1Part 9'' Double Face Body - Top & Bottom - Mitered both ends\",IF(BodyType=5,\" 1Part 12'' Double Face Body - Top & Bottom - Mitered both ends\",\"\")))))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=1,KQ,IF(Body=2,\"\",IF(Body=3,KQ*2,IF(Body=4,\"\",IF(Body=5,\"\")))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=1,Hgt,IF(Body=2,\"\",IF(Body=3,Hgt,IF(Body=4,\"\",IF(Body=5,\"\",\"\")))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(AND(BodyType=1,Body=1),\"1921\"&PPTD,IF(AND(BodyType=2,Body=1),\"1922\"&PPTD,IF(AND(BodyType=3,Body=1),\"1931\"&PPTD,IF(AND(BodyType=4,Body=1),\"1923\"&PPTD,IF(AND(BodyType=5,Body=1),\"1924\"&PPTD,IF(Body=2,\"\",IF(AND(BodyType=1,Body=3),\"1921\"&PPTD,IF(AND(BodyType=2,Body=3),\"1922\"&PPTD,IF(AND(BodyType=3,Body=3),\"1931\"&PPTD,IF(AND(BodyType=4,Body=3),\"1923\"&PPTD,IF(AND(BodyType=5,Body=3),\"1924\"&PPTD,IF(Body=4,\"\",IF(Body=5,\"\")))))))))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(AND(BodyType=1,Body=1),\" 1Part 6'' Single Face Body - One End - Mitered both ends\",IF(AND(BodyType=2,Body=1),\" 1Part 8'' Single Face Body - One End - Mitered both ends\",IF(AND(BodyType=3,Body=1),\" 1Part 6'' Double Face Body - One End - Mitered both ends\",IF(AND(BodyType=4,Body=1),\" 1Part 9'' Double Face Body - One End - Mitered both ends\",IF(AND(BodyType=5,Body=1),\" 1Part 12'' Double Face Body - One End - Mitered both ends\",IF(Body=2,\"\",IF(AND(BodyType=1,Body=3),\" 1Part 6'' Single Face Body - Both Ends - Mitered both ends\",IF(AND(BodyType=2,Body=3),\" 1Part 8'' Single Face Body - Both Ends - Mitered both ends\",IF(AND(BodyType=3,Body=3),\" 1Part 6'' Double Face Body - Both End - Mitered both ends\",IF(AND(BodyType=4,Body=3),\" 1Part 9'' Double Face Body - Both Ends - Mitered both ends\",IF(AND(BodyType=5,Body=3),\" 1Part 12'' Double Face Body - Both Ends - Mitered both ends\",IF(Body=4,\"\",IF(Body=5,\"\")))))))))))))))","v":""}]
[]
[null,"2Part Body"]
[]
[null,"Qty.","Size (in)",null,"x","Part #",null,"  Description"]
[null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=1,\"\",IF(Body=2,\"\",IF(Body=3,\"\",IF(Body=4,KQ*2,IF(Body=5,\"\",\"\")))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=1,\"\",IF(Body=2,\"\",IF(Body=3,\"\",IF(Body=4,Wdt,IF(Body=5,\"\",\"\")))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(Body=1,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=2,\"\",IF(Body=3,\"\",IF(AND(BodyType=1,Body=4),\"1926\"&PPTD,IF(AND(BodyType=2,Body=4),\"1927\"&PPTD,IF(AND(BodyType=3,Body=4),\"1936\"&PPTD,IF(AND(BodyType=4,Body=4),\"1928\"&PPTD,IF(AND(BodyType=5,Body=4),\"1929\"&PPTD,IF(Body=5,\"\")))))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\" Select 2Part Body Only\",IF(Body=1,\"\",IF(Body=2,\"\",IF(Body=3,\"\",IF(AND(BodyType=1,Body=4),\" 2Part 6'' Single Face Body - Top & Bottom - Mitered both ends\",IF(AND(BodyType=2,Body=4),\" 2Part 8'' Single Face Body - Top & Bottom - Mitered both ends\",IF(AND(BodyType=3,Body=4),\" 2Part 6'' Double Face Body - Top & Bottom - Mitered both ends\",IF(AND(BodyType=4,Body=4),\" 2Part 9'' Double Face Body - Top & Bottom - Mitered both ends\",IF(AND(BodyType=5,Body=4),\" 2Part 12'' Double Face Body - Top & Bottom - Mitered both ends\",IF(Body=5,\"\")))))))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," Select 2Part Body Only"]
[null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=1,KQ,IF(Body=2,KQ*2,IF(Body=3,\"\",IF(Body=4,KQ*2,IF(Body=5,\"\")))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(Body=1,Hgt,IF(Body=2,Hgt,IF(Body=3,\"\",IF(Body=4,Hgt,IF(Body=5,\"\",\"\")))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\"\",IF(AND(BodyType=1,Body=1),\"1926\"&PPTD,IF(AND(BodyType=2,Body=1),\"1927\"&PPTD,IF(AND(BodyType=3,Body=1),\"1936\"&PPTD,IF(AND(BodyType=4,Body=1),\"1928\"&PPTD,IF(AND(BodyType=5,Body=1),\"1929\"&PPTD,IF(AND(BodyType=1,Body=2),\"1926\"&PPTD,IF(AND(BodyType=2,Body=2),\"1927\"&PPTD,IF(AND(BodyType=3,Body=2),\"1936\"&PPTD,IF(AND(BodyType=4,Body=2),\"1928\"&PPTD,IF(AND(BodyType=5,Body=2),\"1929\"&PPTD,IF(Body=3,\"\",IF(AND(BodyType=1,Body=4),\"1926\"&PPTD,IF(AND(BodyType=2,Body=4),\"1927\"&PPTD,IF(AND(BodyType=3,Body=4),\"1936\"&PPTD,IF(AND(BodyType=4,Body=4),\"1928\"&PPTD,IF(AND(BodyType=5,Body=4),\"1929\"&PPTD,IF(Body=5,\"\",\"\")))))))))))))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(AND(Body<=3,NOYES=2),\" Select 2Part Body Only\",IF(AND(BodyType=1,Body=1),\" 2Part 6'' Single Face Body - One End - Mitered both ends\",IF(AND(BodyType=2,Body=1),\" 2Part 8'' Single Face Body - One End - Mitered both ends\",IF(AND(BodyType=3,Body=1),\" 2Part 6'' Double Face Body - One End - Mitered both ends\",IF(AND(BodyType=4,Body=1),\" 2Part 9'' Double Face Body - One End - Mitered both ends\",IF(AND(BodyType=5,Body=1),\" 2Part 12'' Double Face Body - One End - Mitered both ends\",IF(AND(BodyType=1,OR(Body=2,Body=4)),\" 2Part 6'' Single Face Body - Both ends - Mitered both ends\",IF(AND(BodyType=2,OR(Body=2,Body=4)),\" 2Part 8'' Single Face Body - Both ends - Mitered both ends\",IF(AND(BodyType=3,OR(Body=2,Body=4)),\" 2Part 6'' Double Face Body - Both ends - Mitered both ends\",IF(AND(BodyType=4,OR(Body=2,Body=4)),\" 2Part 9'' Double Face Body - Both ends - Mitered both ends\",IF(AND(BodyType=5,OR(Body=2,Body=4)),\" 2Part 12'' Double Face Body - Both ends - Mitered both ends\",IF(Body=3,\"\",IF(Body=5,\"\",\"\"))))))))))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[]
[null,"Retainer Type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,"Retainer"]
[null,"2Part Retainer",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1," Retainer Type"]
[]
[" ","Qty.","Size (in)",null,"x","Part #",null,"  Description"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(BodyType<=2,Body=4),KQ*2,IF(AND(BodyType>=3,Body=4),KQ*4,IF(Body=5,KQ*2,\"\"))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body=4,RETTYPE>=1),Wdt+0.03125,IF(AND(Body=5,RETTYPE=1),Wdt+0.305+0.03125,IF(AND(Body=5,RETTYPE>=2),Wdt+0.25+0.03125,\"\"))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(AND(BodyType=3,Body=4,RETTYPE=1)),\"1954\"&PPTD,IF(AND(Body=4,RETTYPE=1),\"1944\"&PPTD,IF(AND(Body>=4,RETTYPE=2),\"1940\"&PPTD,IF(AND(Body>=4,RETTYPE=3),\"1940\"&PPTD,IF(AND(Body>=4,RETTYPE=4),\"1940\"&PPTD,IF(AND(Body>=4,RETTYPE=5),\"1939\"&PPTD,IF(AND(Body=5,RETTYPE=1),\"1954\"&PPTD,\"\"))))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body>=4,RETTYPE=1),\" 2Part Retainer - Top & Bottom - Mitered both ends\",IF(AND(Body>=4,RETTYPE=2),\" 2Part Extended Retainer - Top & Bottom - Mitered both ends\",IF(AND(Body>=4,RETTYPE=3),\" 2Part Extended Retainer - Top & Bottom - Mitered both ends\",IF(AND(Body>=4,RETTYPE=4),\" 2Part Extended Retainer - Top & Bottom - Mitered both ends\",IF(AND(Body>=4,RETTYPE=5),\" 2Part Large Extended Retainer - Top & Bottom - Mitered both ends\",\"\"))))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(AND(BodyType<=2,Body=1,RETTYPE=1)),KQ,IF(AND(AND(BodyType>=3,Body=1,RETTYPE=1)),KQ*2,IF(AND(AND(BodyType<=2,Body=2,RETTYPE=1)),KQ*2,IF(AND(AND(BodyType>=3,Body=2,RETTYPE=1)),KQ*4,IF(AND(AND(BodyType<=2,Body=4,RETTYPE<=2)),KQ*2,IF(AND(AND(BodyType>=3,Body=4,RETTYPE<=2)),KQ*4,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=3)),KQ,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=3)),KQ*2,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=5)),KQ*2,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=5)),KQ*4,IF(AND(Body=5,RETTYPE=1),KQ*2,IF(AND(Body=5,RETTYPE=2),KQ*2,IF(AND(Body=5,RETTYPE=3),KQ,IF(AND(Body=5,RETTYPE=5),KQ*2,\"\")))))))))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(AND(BodyType<=2,Body=1,RETTYPE=1)),Hgt+0.03125,IF(AND(AND(BodyType>=3,Body=1,RETTYPE=1)),Hgt+0.03125,IF(AND(AND(BodyType<=2,Body=2,RETTYPE=1)),Hgt+0.03125,IF(AND(AND(BodyType>=3,Body=2,RETTYPE=1)),Hgt+0.03125,IF(AND(Body=4,RETTYPE=1),Hgt+0.03125,IF(AND(Body=4,RETTYPE=2),Hgt+0.03125,IF(AND(Body=4,RETTYPE=3),Hgt+0.03125,IF(AND(Body=4,RETTYPE=5),Hgt+0.03125,IF(AND(Body=5,RETTYPE=1),Hgt+0.305+0.03125,IF(AND(Body=5,RETTYPE=2),Hgt+0.25+0.03125,IF(AND(Body=5,RETTYPE=3),Hgt+0.25+0.03125,IF(AND(Body=5,RETTYPE=5),Hgt+0.25+0.03125,\"\")))))))))))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(BodyType<=2,RETTYPE=1,OR(Body<=2,Body=4)),\"1944\"&PPTD,IF(AND(AND(BodyType=3,Body<=2,RETTYPE=1)),\"1954\"&PPTD,IF(AND(AND(BodyType=3,Body=4,RETTYPE=1)),\"1954\"&PPTD,IF(AND(BodyType>=4,RETTYPE=1,OR(Body<=2,Body=4)),\"1944\"&PPTD,IF(AND(AND(BodyType<=5,Body=4,RETTYPE=2)),\"1940\"&PPTD,IF(AND(AND(BodyType<=5,Body=4,RETTYPE=3)),\"1940\"&PPTD,IF(AND(AND(BodyType<=5,Body=4,RETTYPE=5)),\"1939\"&PPTD,IF(AND(Body=5,RETTYPE=1),\"1954\"&PPTD,IF(AND(Body=5,RETTYPE=2),\"1940\"&PPTD,IF(AND(Body=5,RETTYPE=3),\"1940\"&PPTD,IF(AND(Body=5,RETTYPE=5),\"1939\"&PPTD,\"\"))))))))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body=1,RETTYPE=1),\" 2Part Retainer - Both Ends - Mitered both ends\",IF(AND(Body=2,RETTYPE=1),\" 2Part Retainer - Both Ends - Mitered both ends\",IF(AND(Body>=4,RETTYPE=1),\" 2Part Retainer - Both Ends - Mitered both ends\",IF(AND(Body>=4,RETTYPE=2),\" 2Part Extended Retainer - Both Ends - Mitered both ends\",IF(AND(Body>=4,RETTYPE=3),\" 2Part Extended Retainer - One End - Mitered both ends\",IF(AND(Body>=4,RETTYPE=5),\" 2Part Large Extended Retainer - Both Ends - Mitered both ends\",\"\")))))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body=5,RETTYPE=3),KQ,IF(AND(Body=5,RETTYPE=4),KQ*2,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=3)),KQ,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=3)),KQ*2,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=4)),KQ*2,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=4)),KQ*4,IF(AND(Body=4,RETTYPE=3),KQ*2,IF(AND(Body=5,RETTYPE=4),KQ*4,IF(AND(Body=5,RETTYPE=3),KQ,IF(AND(Body=5,RETTYPE=4),KQ*2,\"\")))))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body=4,RETTYPE=3),Hgt+0.03125,IF(AND(Body=4,RETTYPE=4),Hgt+0.03125,IF(AND(Body=5,RETTYPE=3),Hgt+0.25+0.03125,IF(AND(Body=5,RETTYPE=4),Hgt+0.25+0.03125,\"\")))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body=4,RETTYPE=3),\"1955\"&PPTD,IF(AND(Body=4,RETTYPE=4),\"1955\"&PPTD,IF(AND(Body=5,RETTYPE=3),\"1955\"&PPTD,IF(AND(Body=5,RETTYPE=4),\"1955\"&PPTD,\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body=4,RETTYPE=3),\"2Part Extened Frame - One End - Mitered both ends\",IF(AND(Body=4,RETTYPE=4),\"2Part Extened Frame - Both Ends - Mitered both ends\",IF(AND(Body=5,RETTYPE=3),\"2Part Extened Frame - One End - Mitered both ends\",IF(AND(Body=5,RETTYPE=4),\"2Part Extened Frame - Both Ends - Mitered both ends\",\"\")))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(AND(BodyType<=2,Body=4,RETTYPE=3)),KQ,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=3)),KQ*2,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=4)),KQ*2,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=4)),KQ*4,IF(AND(Body=5,RETTYPE=3),KQ,IF(AND(Body=5,RETTYPE=4),KQ*2,\"\")))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body=4,RETTYPE=3),Hgt+0.03125,IF(AND(Body=4,RETTYPE=4),Hgt+0.03125,IF(AND(Body=5,RETTYPE=3),Hgt+0.25+0.03125,IF(AND(Body=5,RETTYPE=4),Hgt+0.25+0.03125,\"\")))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body=4,RETTYPE=3),\"1944\"&PPTD,IF(AND(Body=4,RETTYPE=4),\"1944\"&PPTD,IF(AND(Body=5,RETTYPE=3),\"1944\"&PPTD,IF(AND(Body=5,RETTYPE=4),\"1944\"&PPTD,\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Ret=2,\"\",IF(AND(Body=4,RETTYPE=3),\"2Part Retainer - One End - Mitered both ends\",IF(AND(Body=4,RETTYPE=4),\"2Part Retainer - Both Ends - Mitered both ends\",IF(AND(Body=5,RETTYPE=3),\"2Part Retainer - One End - Mitered both ends\",IF(AND(Body=5,RETTYPE=4),\"2Part Retainer - Both Ends - Mitered both ends\",\"\")))))))","v":""}]
[]
[null,"Divider",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1," Divider"]
[]
[null,"2Part Divider",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,false,false]
[null,null,null,null,0,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(HD=TRUE,\" Insert Number of Horizontal Divider(s)\",\"\")))))","v":""},null,null,null,null,null,null,null,null,0,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(VD=TRUE,\" Insert Number of Vertical Divider(s)\",\"\")))))","v":""}]
[]
[null,"Qty.","Size (in)",null,"x","Part #",null,"  Description"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(AND(BodyType<=2,Body<=2,HD=TRUE)),KQ*NHD,IF(AND(AND(BodyType>=3,Body<=2,HD=TRUE)),KQ*NHD*2,IF(AND(AND(BodyType<=2,Body>=4,HD=TRUE)),KQ*NHD,IF(AND(AND(BodyType>=3,Body>=4,HD=TRUE)),KQ*NHD*2,\"\")))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(AND(Body=5,RETTYPE<=4,HD=TRUE)),Wdt-3,IF(AND(AND(Body=5,RETTYPE=5,HD=TRUE)),Wdt-3.75,IF(AND(RETTYPE<=4,HD=TRUE),Wdt-3.25,IF(AND(RETTYPE=5,HD=TRUE),Wdt-2,\"\")))))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(RETTYPE<=4,HD=TRUE),\"1905\"&PPTD,IF(AND(RETTYPE=5,HD=TRUE),\"1905\"&PPTD,\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\" Divider does not integrate with 1Part Bodies on all sides - select one or both end(s) removeable\",IF(AND(RETTYPE<=4,HD=TRUE),\" 2Part Divider - Horizontal - Straight Cut Both Ends\",IF(AND(RETTYPE=5,HD=TRUE),\" 2Part Divider - Horizontal - Straight Cut Both Ends\",\"\")))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," Select Both Ends Removeable"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body=1,VD=TRUE),\"\",IF(AND(AND(BodyType<=2,Body<=2,VD=TRUE)),KQ*NVD,IF(AND(AND(BodyType>=3,Body<=2,VD=TRUE)),KQ*NVD*2,IF(AND(AND(BodyType<=2,Body>=4,VD=TRUE)),KQ*NVD,IF(AND(AND(BodyType>=3,Body>=4,VD=TRUE)),KQ*NVD*2,\"\"))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body=1,VD=TRUE),\"\",IF(AND(AND(Body=5,RETTYPE<=4,VD=TRUE)),Hgt-3,IF(AND(AND(Body=5,RETTYPE=5,VD=TRUE)),Hgt-3.75,IF(AND(RETTYPE<=4,VD=TRUE),Hgt-3.25,IF(AND(RETTYPE=5,VD=TRUE),Hgt-2,\"\"))))))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body=1,VD=TRUE),\"\",IF(AND(RETTYPE<=4,VD=TRUE),\"1905\"&PPTD,IF(AND(RETTYPE=5,VD=TRUE),\"1905\"&PPTD,\"\"))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\" Divider does not integrate with 1Part Bodies on all sides - select one or both end(s) removeable\",IF(AND(Body=1,VD=TRUE),\" Select Both Ends Removeable\",IF(AND(RETTYPE<=4,VD=TRUE),\" 2Part Divider - Vertical - Straight Cut Both Ends\",IF(AND(RETTYPE=5,VD=TRUE),\" 2Part Divider - Vertical - Straight Cut Both Ends\",\"\"))))))))","v":""}]
[]
[null,"Vandal Cover",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1," Vandal Cover"]
[]
[null,"Inner Frame",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1," Frame Type"]
[]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(BodyType<=2,Body=4),KQ*2,IF(AND(BodyType>=3,Body=4),KQ*4,IF(Body=5,KQ*2,\"\"))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(Body=4,Wdt+0.03125,IF(Body=5,Wdt+0.25,\"\")))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=1,\"1960\"&PPTD,IF(INFRM=2,\"1959\"&PPTD,\"\")))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=1,\" 2Part Inner Frame - Top & Bottom - Mitered both ends\",IF(INFRM=2,\" 2Part Large Inner Frame - Top & Bottom - Mitered both ends\",\"\")))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(BodyType<=2,Body=4),KQ*2,IF(AND(BodyType>=3,Body=4),KQ*4,IF(Body=5,KQ*2,\"\"))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(Body=4,Hgt+0.03125,IF(Body=5,Hgt+0.25,\"\")))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=1,\"1960\"&PPTD,IF(INFRM=2,\"1959\"&PPTD,\"\")))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=1,\" 2Part Inner Frame - Both Ends - Mitered both ends\",IF(INFRM=2,\" 2Part Large Inner Frame - Both Ends - Mitered both ends\",\"\")))))","v":""}]
[]
[null,"Outer Frame",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1," Vandal Cover"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1," Hinge"]
[]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(BodyType<=2,Body=4),KQ*2,IF(AND(BodyType>=3,Body=4),KQ*4,IF(Body=5,KQ*2,\"\"))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(OTFRM=1,Hinge=1),IFW-0.875,IF(AND(OTFRM=2,Hinge=1),IFW-1.1875,IF(AND(OTFRM=1,Hinge=2),IFW-1.125,IF(AND(OTFRM=2,Hinge=2),IFW-1.171875)))))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(OTFRM=1,\"1942\"&PPTD,IF(OTFRM=2,\"1941\"&PPTD)))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\" Select 2Part Large Inner Frame\",IF(AND(INFRM=2,OTFRM=1),\" Select 2Part Large Outer Frame\",IF(OTFRM=1,\" 2Part Outer Frame - Top/Bottom - Mitered both ends\",IF(OTFRM=2,\" 2Part Large Outer Frame - Top/Bottom - Mitered both ends\")))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," Select 2Part Large Inner Frame",null,null," Select 2Part Large Outer Frame"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(BodyType<=2,Body=4),KQ*2,IF(AND(BodyType>=3,Body=4),KQ*4,IF(Body=5,KQ*2,\"\"))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(OTFRM=1,Hinge=1),IFH-1.125,IF(AND(OTFRM=2,Hinge=1),IFH-1.171875,IF(AND(OTFRM=1,Hinge=2),IFH-0.875,IF(AND(OTFRM=2,Hinge=2),IFH-1.1875)))))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(OTFRM=1,\"1942\"&PPTD,IF(OTFRM=2,\"1941\"&PPTD)))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\" Select 2Part Large Inner Frame\",IF(AND(INFRM=2,OTFRM=1),\" Select 2Part Large Outer Frame\",IF(OTFRM=1,\" 2Part Outer Frame - Both ends -  Mitered both ends\",IF(OTFRM=2,\" 2Part Large Outer Frame -  Both ends - Mitered both ends\")))))))","v":""}]
[null,"Hinge"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(BodyType=1,KQ*1,IF(BodyType=2,KQ*1,IF(BodyType=3,KQ*2,IF(BodyType=4,KQ*2,IF(BodyType=5,KQ*2))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(Hinge=1,OFH,IF(Hinge=2,OFW)))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(OTFRM=1,\"5996\"&PPTD,IF(OTFRM=2,\"5997\"&PPTD)))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\" Select 2Part Large Inner Frame\",IF(AND(INFRM=2,OTFRM=1),\" Select 2Part Large Outer Frame\",IF(AND(OTFRM=1,Hinge=1),\" 2Part Hinge - Top or Bottom Hinged - 1-1/16'' x .90'' Aluminum Hinge\",IF(AND(OTFRM=2,Hinge=1),\" 2Part Large Hinge - Top or Bottom Hinged - 1-1/16'' x .090'' Aluminum Hinge\",IF(AND(OTFRM=1,Hinge=2),\" 2Part Hinge - Side Hinged - 1-1/2'' x .090'' Aluminum Hinge\",IF(AND(OTFRM=2,Hinge=2),\" 2Part Large Hinge - Side Hinged - 1-1/2'' x .090'' Aluminum Hinge\")))))))))","v":""}]
[]
[]
[]
[]
[]
[null,"BILL OF MATERIALS"]
[]
[null,{"$f":"IF(KQ=0,\"\",AI6&AE4&AE6&AE7&AE9&AE10&AI7)","v":""}]
[]
[]
[null,"Customer  ",null,null,null,{"$f":"IF(Cust=0,\"\",Cust)","v":""},null,null,null,null,null,null,null,null,"Order#   ",null,null,null,{"$f":"IF(Ordnum=0,\"\",Ordnum)","v":""}]
[null,"Kit Quantity  ",null,null,null,{"$f":"IF(KQ=0,\"\",KQ)","v":""},null,"Height  ",null,null,null,{"$f":"IF(Hgt=0,\"\",Hgt)","v":""},null,"Width",null,null,null,{"$f":"IF(Wdt=0,\"\",Wdt)","v":""}]
[]
[null,"Hardware"]
[null,"Body"]
[null,{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(Body<=4,KQ*4,\"\")))","v":""},{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(AND(BodyType=1,Body<=4),\"5981\",IF(AND(BodyType=2,Body<=4),\"5979\",IF(AND(BodyType=3,Body<=4),\"5985\",IF(AND(BodyType=4,Body<=4),\"5978\",IF(AND(BodyType=5,Body<=4),\"5977\",\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(AND(BodyType=1,Body<=4),\" 1Part-2Part 6'' Single Face Body Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (4-3/16'') - One (1) per corner\",IF(AND(BodyType=2,Body<=4),\" 1Part-2Part 8'' Single Face Body Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (6-3/16'') - One (1) per corner\",IF(AND(BodyType=3,Body<=4),\" 1Part-2Part 6'' Double Face Body Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (3-3/4'') - One (1) per corner\",IF(AND(BodyType=4,Body<=4),\" 1Part-2Part 9'' Double Face Body Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (6-5/16'') - One (1) per corner\",IF(AND(BodyType=5,Body<=4),\" 1Part-2Part 12'' Double Face Body Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (9-5/16'') - One (1) per corner\",\"\")))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(Body<=4,KQ*18,\"\")))","v":""},{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(Body<=4,\"5218\",\"\")))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(AND(BodyType<=5,Body<=4),\" Corner Angle Screw - #10 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type AB - Four (4) per corner\",\"\")))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(BodyType=3,\"\",IF(OR(BodyType<=2,BodyType>=4),KQ*8,\"\"))))","v":""},{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(BodyType=3,\"\",IF(OR(BodyType<=2,BodyType>=4),\"5210\",\"\"))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(Body=5,\"\",IF(BodyType=3,\"\",IF(OR(BodyType<=2,BodyType>=4),\" Corner Key  - .120 Stamped Aluminum - Two (2) per corner\",\"\"))))","v":""}]
[null,"Retainer"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(AND(Body=4,Ret=2),\"\",IF(AND(Body<=3,RETTYPE>=2),\"\",IF(AND(BodyType<=2,Body<=4),KQ*4,IF(AND(BodyType>=3,Body<=4),KQ*8,IF(Body=5,KQ*4,\"\")))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(AND(Body=4,Ret=2),\"\",IF(AND(Body<=3,RETTYPE>=2),\"\",IF(AND(BodyType<=2,Body<=4),\"5210\",IF(AND(BodyType>=3,Body<=4),\"5210\",IF(Body=5,\"5210\",\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(AND(Body=4,Ret=2),\"\",IF(AND(Body<=3,RETTYPE>=2),\"\",IF(AND(BodyType<=2,Body<=4),\" Corner Key - .120 Stamped Aluminum - One (1) per corner\",IF(AND(BodyType>=3,Body<=4),\" Corner Key - .120 Stamped Aluminum - Two (2) per corner\",IF(Body=5,\" Corner Key - .120 Stamped Aluminum - One (1) per corner\",\"\")))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(AND(Body>=1,Body<=3),\"\",IF(AND(Body=4,RETTYPE=1),\"\",IF(AND(AND(BodyType<=2,Body=4,RETTYPE>=2)),KQ*4,IF(AND(AND(BodyType>=3,Body=4,RETTYPE>=2)),KQ*8,IF(AND(Body=5,RETTYPE>=2),KQ*4,\"\")))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(AND(Body>=1,Body<=3),\"\",IF(AND(Body=4,RETTYPE=1),\"\",IF(AND(AND(BodyType<=2,Body=4,RETTYPE>=2)),\"5305\",IF(AND(AND(BodyType>=3,Body=4,RETTYPE>=2)),\"5305\",IF(AND(Body=5,RETTYPE>=2),\"5305\",\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(AND(Body>=1,Body<=3),\"\",IF(AND(Body=4,RETTYPE=1),\"\",IF(AND(AND(BodyType<=2,Body=4,RETTYPE>=2)),\" Frame Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (1-1/16'') - One (1) per corner\",IF(AND(AND(BodyType>=3,Body=4,RETTYPE>=2)),\" Frame Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (1-1/16'') - Two (2) per corner\",IF(AND(Body=5,RETTYPE>=2),\" Frame Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (1-1/16'') - One (1) per corner\",\"\")))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Body=3,\"\",IF(AND(Body=4,Ret=2),\"\",IF(Body=5,\"\",IF(AND(AND(BodyType<=2,Body=1,RETTYPE=1)),(VERT1+2)*KQ,IF(AND(AND(BodyType>=3,Body=1,RETTYPE=1)),((VERT1*2)+2)*KQ,IF(AND(AND(BodyType<=2,Body=2,RETTYPE=1)),((VERT1+VERT2)+2)*KQ,IF(AND(AND(BodyType>=3,Body=2,RETTYPE=1)),(((VERT1+VERT2)*2)+2)*KQ,IF(AND(BodyType<=2,Body=4),(TFTBS+2)*KQ,IF(AND(BodyType>=3,Body=4),((TFTBS*2)+2)*KQ,\"\")))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Body=3,\"\",IF(AND(Body=4,Ret=2),\"\",IF(Body=5,\"\",IF(AND(AND(BodyType=3,Body<=2,RETTYPE=1)),\"5290\"&PPTD,IF(AND(AND(BodyType<=2,Body<=2,RETTYPE=1)),\"5290\"&PPTD,IF(AND(AND(BodyType>=3,Body<=2,RETTYPE=1)),\"5290\"&PPTD,IF(AND(Body=4,RETTYPE=1),\"5290\"&PPTD,IF(AND(Body=4,RETTYPE>=2),\"5290\"&PPTD,\"\"))))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Body=3,\"\",IF(AND(Body=4,Ret=2),\"\",IF(Body=5,\"\",IF(AND(AND(BodyType=3,Body<=2,RETTYPE=1)),\" 2Part Retainer Screw - #8 x 1/2'' Sq/Phillips Pan/Countersink Head S.S. Screws - Type A - One (1) every 12'' on center\",IF(AND(Body<=2,RETTYPE=1),\" 2Part Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",IF(AND(Body=4,RETTYPE=1),\" 2Part Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",IF(AND(Body=4,RETTYPE>=2),\" 2Part Extended Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",IF(AND(Body=4,RETTYPE=3),\" 2Part Extended Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",IF(AND(Body=4,RETTYPE=4),\" 2Part Extended Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",IF(AND(Body=4,RETTYPE=5),\" 2Part Large Extended Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",\"\"))))))))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Body=3,\"\",IF(Body=5,\"\",IF(AND(AND(BodyType=3,Body=1,RETTYPE=1)),((VERT1*2)+2)*KQ,IF(AND(AND(BodyType=3,Body=2,RETTYPE=1)),(((VERT1+VERT2)*2)+2)*KQ,IF(AND(AND(BodyType=3,Body=4,RETTYPE=1)),((TFTBS*2)+2)*KQ,\"\")))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Body=3,\"\",IF(Body=5,\"\",IF(AND(AND(BodyType=3,Body<=2,RETTYPE=1)),\"5168\"&PPTD,IF(AND(AND(BodyType=3,Body=4,RETTYPE=1)),\"5168\"&PPTD,\"\"))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Body=3,\"\",IF(Body=5,\"\",IF(AND(AND(BodyType=3,Body<=2,RETTYPE=1)),\" 2Part Retainer Screw - #8 x 1/2'' Sq/Phillips Pan/Countersink Head S.S. Screws - Type A - One (1) every 12'' on center\",IF(AND(AND(BodyType=3,Body=4,RETTYPE=1)),\" 2Part Retainer Screw - #8 x 1/2'' Sq/Phillips Pan/Countersink Head S.S. Screws - Type A - One (1) every 12'' on center\",\"\"))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Body<=3,\"\",IF(AND(AND(BodyType<=2,Body=4,RETTYPE=2)),KQ*6,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=2)),KQ*6,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=3)),KQ*4,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=3)),KQ*6,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=5)),KQ*6,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=5)),KQ*10,IF(AND(Body=5,RETTYPE=2),KQ*10,IF(AND(Body=5,RETTYPE=3),KQ*8,IF(AND(Body=5,RETTYPE=4),KQ*6,IF(AND(Body=5,RETTYPE=5),KQ*10,\"\")))))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Body<=3,\"\",IF(AND(AND(BodyType<=2,Body=4,RETTYPE=2)),\"5241\"&PPTD,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=2)),\"5241\"&PPTD,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=3)),\"5241\"&PPTD,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=3)),\"5241\"&PPTD,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=5)),\"5241\"&PPTD,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=5)),\"5241\"&PPTD,IF(AND(Body=5,RETTYPE>=2),\"5241\"&PPTD,\"\"))))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(Body<=3,\"\",IF(AND(AND(BodyType<=2,Body=4,RETTYPE=2)),\" 2Part Extended Retainer Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - One (1) per corner\",IF(AND(AND(BodyType>=3,Body=4,RETTYPE=2)),\" 2Part Extended Retainer Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - One (1) per corner \",IF(AND(AND(BodyType<=2,Body=4,RETTYPE=3)),\" 2Part Extended Retainer Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - One (1) per corner\",IF(AND(AND(BodyType>=3,Body=4,RETTYPE=3)),\" 2Part Extended Retainer Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - One (1) per corner\",IF(AND(Body=4,RETTYPE=5),\" 2Part Large Extended Retainer Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - One (1) per corner\",IF(AND(Body=5,RETTYPE=2),\" 2Part Extended Retainer Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - Two (2) per corner\",IF(AND(Body=5,RETTYPE=3),\" 2Part Ext. Ret. Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - Two (2) per corner one side\",IF(AND(Body=5,RETTYPE=4),\" 2Part Extended Retainer Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - One (1) per corner\",IF(AND(Body=5,RETTYPE=5),\" 2Part Large Extended Retainer Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - Two (2) per corner\",\"\"))))))))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(AND(AND(BodyType<=2,Body=4,RETTYPE=3)),(VERT1+2)*KQ,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=3)),((VERT1*2)+2)*KQ,IF(AND(AND(BodyType<=2,Body=4,RETTYPE=4)),((VERT1+VERT2)+2)*KQ,IF(AND(AND(BodyType>=3,Body=4,RETTYPE=4)),(((VERT1+VERT2)*2)+2)*KQ,IF(AND(Body=5,RETTYPE=3),(VERT1+2)*KQ,IF(AND(Body=5,RETTYPE=4),((VERT1+VERT2)+2)*KQ,\"\"))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(AND(Body=4,RETTYPE=3),\"5290\"&PPTD,IF(AND(Body=4,RETTYPE=4),\"5290\"&PPTD,IF(AND(Body=5,RETTYPE=3),\"5290\"&PPTD,IF(AND(Body=5,RETTYPE=4),\"5290\"&PPTD,\"\"))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(AND(Body=4,RETTYPE=3),\" 2Part Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",IF(AND(Body=4,RETTYPE=4),\" 2Part Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",IF(AND(Body=5,RETTYPE=3),\" 2Part Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",IF(AND(Body=5,RETTYPE=4),\" 2Part Retainer Screw - #8 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type A - One (1) every 12'' on center\",\"\"))))))","v":""}]
[null,"Divider"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(AND(BodyType<=2,Body<=2,HD=TRUE)),KQ*NHD*4,IF(AND(AND(BodyType>=3,Body<=2,HD=TRUE)),KQ*NHD*4*2,IF(AND(AND(BodyType<=2,Body=4,HD=TRUE)),KQ*NHD*4,IF(AND(AND(BodyType>=3,Body=4,HD=TRUE)),KQ*NHD*4*2,IF(AND(Body=5,HD=TRUE),KQ*NHD*4,\"\"))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body<=2,HD=TRUE),\"5300\",IF(AND(Body=4,HD=TRUE),\"5300\",IF(AND(Body=5,HD=TRUE),\"5300\",\"\"))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\" Divider does not integrate with 1Part Bodies on all sides - select one or both end(s) removeable\",IF(AND(Body<=2,HD=TRUE),\" 2Part Divider Angle - Two (2) Per End -( Horizontal Divider/s)\",IF(AND(Body=4,HD=TRUE),\" 2Part Divider Angle - Two (2) Per End - (Horizontal Divider/s)\",IF(AND(Body=5,HD=TRUE),\" 2Part Divider Angle - Two (2) Per End - (Horizontal Divider/s)\",\"\"))))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," Divider does not integrate with 1Part Bodies on all sides - select one or both end(s) removeable"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\"\",IF(AND(AND(BodyType<=2,Body<=2,VD=TRUE)),KQ*NVD*4,IF(AND(AND(BodyType>=3,Body<=2,VD=TRUE)),KQ*NVD*4*2,IF(AND(AND(BodyType<=2,Body=4,VD=TRUE)),KQ*NVD*4,IF(AND(AND(BodyType>=3,Body=4,VD=TRUE)),KQ*NVD*4*2,IF(AND(Body=5,VD=TRUE),KQ*NVD*4,\"\"))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body<=2,VD=TRUE),\"5300\",IF(AND(Body=4,VD=TRUE),\"5300\",IF(AND(Body=5,VD=TRUE),\"5300\",\"\"))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body<=2,VD=TRUE),\" 2Part Divider Angle - Two (2) Per End - (Vertical Divider/s)\",IF(AND(Body=4,VD=TRUE),\" 2Part Divider Angle - Two (2) Per End - (Vertical Divider/s)\",IF(AND(Body=5,VD=TRUE),\" 2Part Divider Angle - Two (2) Per End - (Vertical Divider/s)\",\"\"))))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(AND(BodyType<=2,Body<=2,HD=TRUE)),((6*NHD)+2)*KQ,IF(AND(AND(BodyType>=3,Body<=2,HD=TRUE)),(((6*NHD)*2)+2)*KQ,IF(AND(AND(BodyType<=2,Body=4,HD=TRUE)),((6*NHD)+2)*KQ,IF(AND(AND(BodyType>=3,Body=4,HD=TRUE)),(((6*NHD)*2)+2)*KQ,IF(AND(Body=5,HD=TRUE),((6*NHD)+2)*KQ,\"\"))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body<=2,HD=TRUE),\"5218\",IF(AND(Body=4,HD=TRUE),\"5218\",IF(AND(Body=5,HD=TRUE),\"5218\",\"\"))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body<=2,HD=TRUE),\" 2Part Divider Angle Screw - #10 x 1/2'' Sq/Phillips Pan Head S.S. - Type AB - Three (3) Per End -( Horizontal Divider/s)\",IF(AND(Body=4,HD=TRUE),\" 2Part Divider Angle Screw - #10 x 1/2'' Sq/Phillips Pan Head S.S. - Type AB - Three (3) Per End - (Horizontal Divider/s)\",IF(AND(Body=5,HD=TRUE),\" 2Part Divider Angle - #10 x 1/2'' Sq/Phillips Pan Head S.S. - Type AB - Three (3) Per End - (Horizontal Divider/s)\",\"\"))))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\"\",IF(AND(AND(BodyType<=2,Body<=2,VD=TRUE)),((6*NVD)+2)*KQ,IF(AND(AND(BodyType>=3,Body<=2,VD=TRUE)),(((6*NVD)*2)+2)*KQ,IF(AND(AND(BodyType<=2,Body=4,VD=TRUE)),((6*NVD)+2)*KQ,IF(AND(AND(BodyType>=3,Body=4,VD=TRUE)),(((6*NVD)*2)+2)*KQ,IF(AND(Body=5,VD=TRUE),((6*NVD)+2)*KQ,\"\"))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body<=2,VD=TRUE),\"5218\",IF(AND(Body=4,VD=TRUE),\"5218\",IF(AND(Body=5,VD=TRUE),\"5218\",\"\"))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(VD=FALSE,\"\",IF(Body=3,\"\",IF(AND(Body<=2,VD=TRUE),\" 2Part Divider Angle Screw - #10 x 1/2'' Sq/Phillips Pan Head S.S. - Type AB - Three (3) Per End -( Vertical Divider/s)\",IF(AND(Body=4,VD=TRUE),\" 2Part Divider Angle Screw - #10 x 1/2'' Sq/Phillips Pan Head S.S. - Type AB - Three (3) Per End - (Vertical Divider/s)\",IF(AND(Body=5,VD=TRUE),\" 2Part Divider Angle - #10 x 1/2'' Sq/Phillips Pan Head S.S. - Type AB - Three (3) Per End - (Vertical Divider/s)\",\"\"))))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(VD=FALSE,NVD=0),\"\",IF(AND(AND(BodyType<=2,Body<=2,HD=TRUE)),KQ*DVJ*4,IF(AND(AND(BodyType>=3,Body<=2,HD=TRUE)),KQ*DVJ*4*2,IF(AND(AND(BodyType<=2,Body=4,HD=TRUE)),KQ*DVJ*4,IF(AND(AND(BodyType>=3,Body=4,HD=TRUE)),KQ*DVJ*4*2,IF(AND(Body=5,HD=TRUE),KQ*DVJ*4,\"\")))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(VD=FALSE,NVD=0),\"\",IF(AND(Body<=2,HD=TRUE),\"5300\",IF(AND(Body=4,HD=TRUE),\"5300\",IF(AND(Body=5,HD=TRUE),\"5300\",\"\")))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(VD=FALSE,NVD=0),\"\",IF(AND(Body<=2,HD=TRUE),\" 2Part Divider Angle - Four (4) Per Joint\",IF(AND(Body=4,HD=TRUE),\" 2Part Divider Angle - Four (4) Per Joint\",IF(AND(Body=5,HD=TRUE),\" 2Part Divider Angle - Four (4) Per Joint\",\"\")))))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"NHD*NVD","v":0}," Number of Divider Joints"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(VD=FALSE,NVD=0),\"\",IF(AND(AND(BodyType<=2,Body<=2,HD=TRUE)),((4*DVJ)*2)*KQ,IF(AND(AND(BodyType>=3,Body<=2,HD=TRUE)),(((4*DVJ)*2)+2)*KQ,IF(AND(AND(BodyType<=2,Body=4,HD=TRUE)),((4*DVJ)+2)*KQ,IF(AND(AND(BodyType>=3,Body=4,HD=TRUE)),(((4*DVJ)*2)+2)*KQ,IF(AND(Body=5,HD=TRUE),((4*DVJ)+2)*KQ,\"\")))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(VD=FALSE,NVD=0),\"\",IF(AND(Body<=2,HD=TRUE),\"5218\",IF(AND(Body=4,HD=TRUE),\"5218\",IF(AND(Body=5,HD=TRUE),\"5218\",\"\")))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=2,\"\",IF(NoYes2=1,\"\",IF(HD=FALSE,\"\",IF(Body=3,\"\",IF(AND(VD=FALSE,NVD=0),\"\",IF(AND(Body<=2,HD=TRUE),\" 2Part Divider Angle Screws - #10 x 1/2'' Sq/Phillips Pan Head S.S. - Type AB - Four (4) Per Joint\",IF(AND(Body=4,HD=TRUE),\" 2Part Divider Angle Screw - #10 x 1/2'' Sq/Phillips Pan Head S.S. - Type AB - Four (4) Per Joint\",IF(AND(Body=5,HD=TRUE),\" 2Part Divider Angle Screw - #10 x 1/2'' Sq/Phillips Pan Head S.S. - Type AB - Four (4) Per Joint\",\"\")))))))))","v":""}]
[null,"Inner Frame"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(AND(BodyType<=2,Body=4,INFRM>=1)),KQ*4,IF(AND(AND(BodyType>=3,Body=4,INFRM>=1)),KQ*8,IF(AND(Body=5,INFRM>=1),KQ*4,\"\"))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(OTFRM=1,\"5210\",IF(OTFRM=2,\"5210\",\"\")))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=1,\" Corner Key - .120'' Stamped Aluminum - One (1) per corner\",IF(INFRM=2,\" Corner Key - .120'' Stamped Aluminum - One (1) per corner\",\"\")))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=1,\"\",IF(AND(AND(BodyType<=2,Body=4,INFRM=2)),KQ*4,IF(AND(AND(BodyType>=3,Body=4,INFRM=2)),KQ*8,IF(AND(Body=5,INFRM=2),KQ*4,\"\")))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=1,\"\",IF(INFRM=2,\"5305\",\"\")))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=1,\"\",IF(INFRM=2,\" Frame Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (1-1/16'') Aluminum Angle - One (1) per corner\",\"\")))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=2,\"\",IF(AND(BodyType<=2,Body=4),KQ*6,IF(AND(BodyType>=3,Body=4),KQ*10,IF(Body=5,KQ*6,\"\")))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=2,\"\",IF(INFRM=1,\"5241\"&PPTD,\"\")))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(INFRM=2,\"\",IF(INFRM=1,\" Corner Screw - #8 x 3/4'' Sq/Phillips Counter Sink S.S. Screw - Type A - One (1) per corner\",\"\")))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(Body=5,\"\",IF(AND(AND(BodyType<=2,Body=4,INFRM>=1)),(TFTBS+2)*KQ,IF(AND(AND(BodyType>=3,Body=4,INFRM>=1)),((TFTBS*2)+2)*KQ,\"\"))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(AND(AND(BodyType>=1,Body=4,INFRM>=1)),\"5290\"&PPTD,\"\")))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(Body=5,\"\",IF(AND(Body=4,INFRM>=1),\"  Inner Frame to Body Screw - #8 x 1/2'' Sq/Phil Pan Head Steel Zinc Screw - Type A - One (1) every 12'' on center\")))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"INT(Hgt/12)+1","v":1},{"$f":"INT(Wdt/12)+1","v":1},{"$f":"INT(Hgt/12)+1","v":1},{"$f":"INT(Wdt/12)+1","v":1},{"$f":"SUM(AE97:AH97)","v":4}," Retainer Screws"]
[null,"Outer Frame"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(OTFRM=1,\"\",IF(AND(AND(BodyType<=2,Body=4,OTFRM=2)),KQ*4,IF(AND(AND(BodyType>=3,Body=4,OTFRM=2)),KQ*8,IF(AND(Body=5,OTFRM=2),KQ*4,\"\")))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(OTFRM=1,\"\",IF(AND(Body=4,OTFRM=2),\"5210\",IF(AND(Body=5,OTFRM=2),\"5210\",\"\"))))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\" Select 2Part Large Inner Frame\",IF(AND(INFRM=2,OTFRM=1),\" Select 2Part Large Outer Frame\",IF(OTFRM=1,\"\",IF(AND(Body>=4,OTFRM=2),\" Corner Key - .120'' Stamped Aluminum - One (1) per corner\",\"\")))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(OTFRM=2,\"\",IF(AND(AND(BodyType<=2,Body=4,OTFRM=1)),KQ*8,IF(AND(AND(BodyType>=3,Body=4,OTFRM=1)),KQ*16,IF(AND(Body=5,OTFRM=1),KQ*8,\"\")))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(OTFRM=2,\"\",IF(AND(Body>=4,OTFRM=1),\"5975\",\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(OTFRM=2,\"\",IF(AND(Body>=4,OTFRM=1),\" Outer Frame Corner Angle - 2'' x 2'' x 1/8'' (3/8'') - Two (2) per corner\",\"\")))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(OTFRM=1,\"\",IF(AND(AND(BodyType<=2,Body=4,OTFRM=2)),KQ*8,IF(AND(AND(BodyType>=3,Body=4,OTFRM=2)),KQ*16,IF(AND(Body=5,OTFRM=2),8*KQ,\"\")))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Body=4,OTFRM=2),\"5305\",IF(AND(Body=5,OTFRM=2),\"5305\",\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Body=4,OTFRM=2),\" Frame Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (1-1/16'') Aluminum Angle - Two (2) per corner\",IF(AND(Body=5,OTFRM=2),\" Frame Corner Angle - 1-3/4'' x 1-3/4'' x 1/4'' (1-1/16'') Aluminum Angle - Two (2) per corner\",\"\")))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(AND(BodyType<=2,Body=4,OTFRM=1)),KQ*18,IF(AND(AND(BodyType>=3,Body=4,OTFRM=1)),KQ*34,IF(AND(AND(BodyType<=2,Body=4,OTFRM=2)),KQ*10,IF(AND(AND(BodyType>=3,Body=4,OTFRM=2)),KQ*18,IF(AND(Body=5,OTFRM=1),KQ*18,IF(AND(Body=5,OTFRM=2),KQ*10,\"\")))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Body>=4,OTFRM=1),\"5990\",IF(AND(Body>=4,OTFRM=2),\"5990\",\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Body>=4,OTFRM=1),\" Outer Frame Corner Angle Screw - #8 x 3/8'' Sq/Phillips Counter Sunk S.S. Screw - Type A - Four (4) per corner\",IF(AND(Body>=4,OTFRM=2),\" Frame Corner Angle Screw - #8 x 3/8'' Sq/Phillips Counter Sunk S.S. Screw - Type A - Two (2) per corner\")))))))","v":""}]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(AND(BodyType<=2,Body=4,OTFRM=2)),KQ*10,IF(AND(AND(BodyType>=3,Body=4,OTFRM=2)),KQ*18,IF(AND(Body=5,OTFRM=2),KQ*10,\"\"))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Body>=4,OTFRM=2),\"5218\",\"\"))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Body>=4,OTFRM=2),\" Frame Corner Angle Screw - #10 x 1/2'' Sq/Phillips Pan Head S.S. Screw - Type AB - Two (2) per corner\",\"\"))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"`"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(AND(BodyType<=2,Body=4,OTFRM>=1)),KQ*NumLocks,IF(AND(AND(BodyType>=3,Body=4,OTFRM>=1)),(NumLocks*2)*KQ,IF(AND(Body=5,OTFRM>=1),KQ*NumLocks,\"\"))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Body>=4,OTFRM=1),\"5994\",IF(AND(Body>=4,OTFRM=2),\"5993\",\"\")))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(AND(Body>=4,OTFRM=1,NumLocks=1)),\" 2Part Lock - One (1) per Outer Frame\",IF(AND(AND(Body>=4,OTFRM=1,NumLocks=2)),\" 2Part Lock - Two (2) per Outer Frame\",IF(AND(AND(Body>=4,OTFRM=2,NumLocks=1)),\" 2Part Large Lock - One (1) per Outer Frame\",IF(AND(AND(Body>=4,OTFRM=2,NumLocks=2)),\" 2Part Large Lock - Two (2) per Outer Frame\",\"\")))))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Wdt<=60,Hinge=1),1,IF(AND(Wdt>=61,Hinge=1),2,IF(AND(Hgt<=60,Hinge=2),1,IF(AND(Hgt>=61,Hinge=2),2)))))))))","v":""},"Locks"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(AND(BodyType<=2,Body=4,OTFRM=1)),1,IF(AND(AND(BodyType>=3,Body=4,OTFRM=1)),1,IF(AND(Body=5,OTFRM=1),1,\"\"))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Body>=4,OTFRM=1),\"5992\",\"\"))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=1,OTFRM=2),\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(Body>=4,OTFRM=1),\" 2Part Lock Wrench\",\"\"))))))","v":""}]
[null,"Hinge"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(AND(AND(BodyType<=2,Body=4,OTFRM=2,Hinge=1))),(((((Wdt-36)/6)+12)*2)+2)*KQ,IF(AND(AND(AND(BodyType>=3,Body=4,OTFRM=2,Hinge=1))),((((((Wdt-36)/6)+12)*2)*2)+2)*KQ,IF(AND(AND(AND(BodyType<=2,Body=4,OTFRM=2,Hinge=2))),(((((Hgt-36)/6)+12)*2)+2)*KQ,IF(AND(AND(AND(BodyType>=3,Body=4,OTFRM=2,Hinge=2))),((((((Hgt-36)/6)+12)*2)*2)+2)*KQ,IF(AND(AND(Body=5,OTFRM=2,Hinge=1)),(((((Wdt-36)/6)+12)*2)+2)*KQ,IF(AND(AND(Body=5,OTFRM=2,Hinge=2)),(((((Hgt-36)/6)+12)*2)+2)*KQ,\"\"))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=2,OTFRM=1),\"\",IF(AND(OTFRM=2,Hinge=1),\"5990\",IF(AND(OTFRM=2,Hinge=2),\"5990\",\"\"))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(Body<=3,\"\",IF(AND(INFRM=2,OTFRM=1),\" Select 2Part Large Outer Frame\",IF(AND(OTFRM=2,Hinge=1),\"2Part Large Hinge Screw - #8 x 3/8'' Sq/Phillips Counter Sunk S.S. Screw - Type-A\",IF(AND(OTFRM=2,Hinge=2),\"2Part Large Hinge Screw - #8 x 3/8'' Sq/Phillips Counter Sunk S.S. Screw - Type-A\",\"\"))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," See Gas Support Placement ''A'' Instruction Sheet"]
[null,"Gas Support",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," See Gas Support Placement ''B'' Instruction Sheet"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(AND(INFRM=1,OTFRM=1),\"\",IF(AND(INFRM=1,OTFRM=2),\"##\",IF(AND(INFRM=2,OTFRM=1),\"##\",IF(Hinge=2,\"\",IF(AND(Body=5,OTFRM=2),1*KQ,IF(AND(BodyType<=2,OTFRM=2),KQ*1,IF(AND(BodyType=3,OTFRM=2),KQ*2,IF(AND(BodyType=4,OTFRM=2),KQ*2,IF(AND(BodyType=5,OTFRM=2),KQ*2,IF(AND(BodyType>=6,OTFRM=2),KQ*1,\"\"))))))))))))","v":""},{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(AND(INFRM=1,OTFRM=1),\"\",IF(AND(INFRM=1,OTFRM=2),\"##\",IF(AND(INFRM=2,OTFRM=1),\"##\",IF(Hinge=2,\"\",IF(AND(INFRM=2,OTFRM=2),'Gas Support'!$C$39)))))))","v":""},null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(AND(INFRM=1,OTFRM=1),\"\",IF(AND(INFRM=1,OTFRM=2),\"##\",IF(AND(INFRM=2,OTFRM=1),\"##\",IF(Hinge=2,\"\",IF(AND(INFRM=2,OTFRM=2),\" Gas Supports - Two (2) Per Face\",\"\")))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," See Gas Support Placement ''C'' Instruction Sheet"]
[null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(AND(INFRM=1,OTFRM=1),\"\",IF(AND(INFRM=1,OTFRM=2),\"##\",IF(AND(INFRM=2,OTFRM=1),\"##\",IF(Hinge=2,\"\",IF(AND(INFRM=2,OTFRM=2),'Gas Support'!$C$61,\"\")))))))","v":""},null,null,{"$f":"IF(KQ=0,\"\",IF(NOYES=1,\"\",IF(AND(INFRM=1,OTFRM=1),\"\",IF(AND(INFRM=1,OTFRM=2),\"##\",IF(AND(INFRM=2,OTFRM=1),\"##\",IF(Hinge=2,\"\",IF(GSPLMT=\"A\",\" See Gas Support Placement ''A'' Instruction Sheet\",IF(GSPLMT=\"B\",\" See Gas Support Placement ''B'' Instruction Sheet\",IF(GSPLMT=\"C\",\" See Gas Support Placement ''C'' Instruction Sheet\",\"\")))))))))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A","B","C"]
[null,"Hardware Summary"]
[]
[null,null,5985,null,{"$f":"SUMIF(C76:C110,C113,B76:B110)","v":0},null,"5290P",null,{"$f":"SUMIF(C76:C110,G113,B76:B110)","v":0},null,5990,null,{"$f":"SUMIF(C76:C110,K113,B76:B110)","v":0},null,5981,null,{"$f":"SUMIF(C76:C110,O113,B76:B110)","v":0},null,5168,null,{"$f":"SUMIF(C76:C110,S113,B76:B110)","v":0}]
[null,null,5218,null,{"$f":"SUMIF(C76:C110,C114,B76:B110)","v":0},null,"5241P",null,{"$f":"SUMIF(C76:C110,G114,B76:B110)","v":0},null,5993,null,{"$f":"SUMIF(C76:C110,K114,B76:B110)","v":0},null,5979,null,{"$f":"SUMIF(C76:C110,O114,B76:B110)","v":0},null,5975,null,{"$f":"SUMIF(C76:C110,S114,B76:B110)","v":0}]
[null,null,5210,null,{"$f":"SUMIF(C76:C110,C115,B76:B110)","v":0},null,5290,null,{"$f":"SUMIF(C76:C110,G115,B76:B110)","v":0},null,5992,null,{"$f":"SUMIF(C76:C110,K115,B76:B110)","v":0},null,5978,null,{"$f":"SUMIF(C76:C110,O115,B76:B110)","v":0},null,5300,null,{"$f":"SUMIF(C77:C111,S115,B77:B111)","v":0}]
[null,null,5305,null,{"$f":"SUMIF(C76:C110,C116,B76:B110)","v":0},null,5241,null,{"$f":"SUMIF(C76:C110,G116,B76:B110)","v":0},null,5994,null,{"$f":"SUMIF(C76:C110,K116,B76:B110)","v":0},null,5977,null,{"$f":"SUMIF(C76:C110,O116,B76:B110)","v":0}]

{"sheet":"Gas Support","index":1,"n_rows":61,"n_cols":13,"rows_kept":61,"cut":false,"hidden":true,"merged":[[60,0,60,1],[20,0,20,1],[22,0,22,1],[38,0,38,1],[42,0,42,1],[44,0,44,1]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"HT","Width"]
["Actual Cabinet Size",null,{"$f":"[0]!Hgt","v":0},{"$f":"[0]!Wdt","v":0},null,null,{"$f":"IF(AH>=90,\"\",IF(AH>=84,84,IF(AH>=78,78,IF(AH>=72,72,IF(AH>=66,66,IF(AH>=60,60,IF(AH>=54,54,IF(AH>=48,48,IF(AH>=42,42,IF(AH>=36,36,IF(AH>=30,30,IF(AH>=24,24))))))))))))","v":false}]
[]
["Nominal Cabinet Size",null,{"$f":"G21","v":false},{"$f":"G23","v":false},null,null,{"$f":"IF(AW>=150,\"\",IF(AW>=144,144,IF(AW>=132,132,IF(AW>=120,120,IF(AW>=108,108,IF(AW>=96,96,IF(AW>=84,84,IF(AW>=72,72,IF(AW>=60,60,IF(AW>=48,48,IF(AW>=36,36)))))))))))","v":false}]
[]
[null,null,null,"WIDTH"]
[null,null,null,36,48,60,72,84,96,108,120,132,144]
[null,"HT",24,"K5933-30","K5933-30","K5933-40","K5933-40","K5933-50","K5933-50","K5933-50","K5933-60","K5933-60","K5933-70"]
[null,null,30,"K5934-30","K5934-30","K5934-30","K5934-40","K5934-40","K5934-40","K5934-50","K5934-50","K5934-50","K5934-60"]
[null,null,36,"K5934-30","K5934-30","K5934-40","K5934-50","K5934-50","K5934-60","K5934-60","K5934-70","K5934-70","K5934-70"]
[null,null,42,"K5934-40","K5934-50","K5934-50","K5934-60","K5934-60","K5934-70","K5934-80","K5934-80","K5934-90","K5934-90"]
[null,null,48,"K5934-50","K5934-60","K5934-60","K5934-70","K5934-80","K5934-90","K5934-90","K5934-100","K5934-110","K5934-110"]
[null,null,54,"K5934-60","K5934-70","K5934-80","K5934-80","K5934-90","K5934-100","K5934-110","K5934-120","K5934-130","K5934-140"]
[null,null,60,"K5934-70","K5934-80","K5934-90","K5934-100","K5934-110","K5934-120","K5934-130","K5934-140","K5934-160","K5934-170"]
[null,null,66,"K5934-80","K5934-90","K5934-100","K5934-120","K5934-130","K5934-140","K5934-150","K5934-170","K5934-180","K5934-110"]
[null,null,72,"K5934-90","K5934-100","K5934-120","K5934-130","K5934-150","K5934-160","K5934-180","K5934-110","K5934-110","K5934-120"]
[null,null,78,"K5934-60","K5934-70","K5934-80","K5934-80","K5934-90","K5934-100","K5934-110","K5934-120","K5934-130","K5934-140"]
[null,null,84,"K5934-60","K5934-70","K5934-80","K5934-90","K5934-100","K5934-120","K5934-130","K5934-140","K5934-150","K5934-160"]
[]
["Gas Support Required",null,{"$f":"INDEX(D27:M37,MATCH(HT,C27:C37,0),MATCH(WTH,D26:M26,0))","v":{"$error":"#N/A"}}]
[]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(AH>=90,\"\",IF(AH>=84,84,IF(AH>=78,78,IF(AH>=72,72,IF(AH>=66,66,IF(AH>=60,60,IF(AH>=54,54,IF(AH>=48,48,IF(AH>=42,42,IF(AH>=36,36,IF(AH>=30,30,IF(AH>=24,24))))))))))))","v":false}]
[]
["Nominal Cabinet Size",null,{"$f":"G43","v":false},{"$f":"G45","v":false},null,null,{"$f":"IF(AW>=150,\"\",IF(AW>=144,144,IF(AW>=132,132,IF(AW>=120,120,IF(AW>=108,108,IF(AW>=96,96,IF(AW>=84,84,IF(AW>=72,72,IF(AW>=60,60,IF(AW>=48,48,IF(AW>=36,36)))))))))))","v":false}]
[]
[null,null,null,"WIDTH"]
[null,null,null,36,48,60,72,84,96,108,120,132,144]
[null,"HT",24,"A","A","A","A","A","A","A","A","A","A"]
[null,null,30,"B","B","B","B","B","B","B","B","B","B"]
[null,null,36,"B","B","B","B","B","B","B","B","B","B"]
[null,null,42,"B","B","B","B","B","B","B","B","B","B"]
[null,null,48,"B","B","B","B","B","B","B","B","B","B"]
[null,null,54,"B","B","B","B","B","B","B","B","B","B"]
[null,null,60,"B","B","B","B","B","B","B","B","B","B"]
[null,null,66,"B","B","B","B","B","B","B","B","B","C"]
[null,null,72,"B","B","B","B","B","B","B","C","C","C"]
[null,null,78,"C","C","C","C","C","C","C","C","C","C"]
[null,null,84,"C","C","C","C","C","C","C","C","C","C"]
[]
["Gas Support Placement",null,{"$f":"INDEX(D49:M59,MATCH(HT,C49:C59,0),MATCH(WTH,D48:M48,0))","v":{"$error":"#N/A"}}]

{"sheet":"GS Placement A","index":2,"n_rows":70,"n_cols":13,"rows_kept":70,"cut":false,"hidden":false,"merged":[[0,1,0,13],[1,1,4,13],[5,1,6,13],[73,1,76,13],[68,8,68,9],[67,8,67,9]]}
[null,"S  I  G  N  C  O  M  P       S  Y  S  T  E  M  S      A  N  D      E  X  T  R  U  S  I  O  N  S"]
[]
[]
[]
[]
[null,"  2Part Large Vandal Cover and Large Vandal Cover"]
[]
[]
[null,null,"Gas Support Placement and Poundage Table:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Weight table for door in lbs."]
[]
[null,null,null,"Width"]
[null,null,"Height",36,48,60,72,84,96,108,120,132,144]
[null,null,24,16,20,24,28,32,37,41,45,49,53]
[null,null,30,19,23,28,33,37,42,47,51,56,60]
[null,null,36,21,26,32,37,42,47,52,58,63,68]
[null,null,42,24,30,35,41,47,53,58,64,70,76]
[null,null,48,26,33,39,45,52,58,64,70,77,83]
[null,null,54,29,36,43,50,56,63,70,77,84,91]
[null,null,60,32,39,46,54,61,69,76,83,91,98]
[null,null,66,34,42,50,58,66,74,82,90,98,106]
[null,null,72,37,45,54,62,71,79,88,96,105,113]
[null,null,78,39,48,58,67,76,85,94,103,112,121]
[null,null,84,42,52,61,71,80,90,100,109,119,128]
[]
[null,null,"Poundage per Gas Support in lbs. (2 Gas Supports per door)"]
[]
[null,null,null,"Width"]
[null,null,"Height",36,48,60,72,84,96,108,120,132,144]
[null,null,24,30,30,40,40,50,50,50,60,60,70]
[null,null,30]
[null,null,36]
[null,null,42]
[null,null,48]
[null,null,54]
[null,null,60]
[null,null,66]
[null,null,72]
[null,null,78]
[null,null,84]
[]
[null,null,null,null,"Placement \"A\" #5933 Gas Support",null,null,null,"Normal",null,"Stock Item"]
[null,null,null,null,"Placement \"B\" #5934 Gas Support",null,null,null,"Bold-Italic",null,"Non-Stock Item (Special Order)"]
[null,null,null,null,"Placement \"C\" #5934 Gas Support"]

{"sheet":"GS Placement B","index":3,"n_rows":70,"n_cols":13,"rows_kept":70,"cut":false,"hidden":false,"merged":[[0,1,0,13],[1,1,4,13],[5,1,6,13],[73,1,76,13],[67,8,67,9],[68,8,68,9]]}
[null,"S  I  G  N  C  O  M  P       S  Y  S  T  E  M  S      A  N  D      E  X  T  R  U  S  I  O  N  S"]
[]
[]
[]
[]
[null,"  2Part Large Vandal Cover and Large Vandal Cover"]
[]
[]
[null,null,"Gas Support Placement and Poundage Table:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Weight table for door in lbs."]
[]
[null,null,null,"Width"]
[null,null,"Height",36,48,60,72,84,96,108,120,132,144]
[null,null,24,16,20,24,28,32,37,41,45,49,53]
[null,null,30,19,23,28,33,37,42,47,51,56,60]
[null,null,36,21,26,32,37,42,47,52,58,63,68]
[null,null,42,24,30,35,41,47,53,58,64,70,76]
[null,null,48,26,33,39,45,52,58,64,70,77,83]
[null,null,54,29,36,43,50,56,63,70,77,84,91]
[null,null,60,32,39,46,54,61,69,76,83,91,98]
[null,null,66,34,42,50,58,66,74,82,90,98,106]
[null,null,72,37,45,54,62,71,79,88,96,105,113]
[null,null,78,39,48,58,67,76,85,94,103,112,121]
[null,null,84,42,52,61,71,80,90,100,109,119,128]
[]
[null,null,"Poundage per Gas Support in lbs. (2 Gas Supports per door)"]
[]
[null,null,null,"Width"]
[null,null,"Height",36,48,60,72,84,96,108,120,132,144]
[null,null,24]
[null,null,30,30,30,30,40,40,40,50,50,50,60]
[null,null,36,30,30,40,50,50,60,60,70,70,70]
[null,null,42,40,50,50,60,60,70,80,80,90,90]
[null,null,48,50,60,60,70,80,90,90,100,110,110]
[null,null,54,60,70,80,80,90,100,110,120,130,140]
[null,null,60,70,80,90,100,110,120,130,140,160,170]
[null,null,66,80,90,100,120,130,140,150,170,180]
[null,null,72,90,100,120,130,150,160,180]
[null,null,78]
[null,null,84]
[]
[null,null,null,null,"Placement \"A\" #5933 Gas Support",null,null,null,"Normal",null,"Stock Item"]
[null,null,null,null,"Placement \"B\" #5934 Gas Support",null,null,null,"Bold-Italic",null,"Non-Stock Item (Special Order)"]
[null,null,null,null,"Placement \"C\" #5934 Gas Support"]

{"sheet":"GS Placement C","index":4,"n_rows":71,"n_cols":13,"rows_kept":71,"cut":false,"hidden":false,"merged":[[0,1,0,13],[1,1,4,13],[5,1,6,13],[73,1,76,13],[68,8,68,9],[69,8,69,9]]}
[null,"S  I  G  N  C  O  M  P       S  Y  S  T  E  M  S      A  N  D      E  X  T  R  U  S  I  O  N  S"]
[]
[]
[]
[]
[null,"  2Part Large Vandal Cover and Large Vandal Cover"]
[]
[]
[null,null,"Gas Support Placement and Poundage Table:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Weight table for door in lbs."]
[]
[null,null,null,"Width"]
[null,null,"Height",36,48,60,72,84,96,108,120,132,144]
[null,null,24,16,20,24,28,32,37,41,45,49,53]
[null,null,30,19,23,28,33,37,42,47,51,56,60]
[null,null,36,21,26,32,37,42,47,52,58,63,68]
[null,null,42,24,30,35,41,47,53,58,64,70,76]
[null,null,48,26,33,39,45,52,58,64,70,77,83]
[null,null,54,29,36,43,50,56,63,70,77,84,91]
[null,null,60,32,39,46,54,61,69,76,83,91,98]
[null,null,66,34,42,50,58,66,74,82,90,98,106]
[null,null,72,37,45,54,62,71,79,88,96,105,113]
[null,null,78,39,48,58,67,76,85,94,103,112,121]
[null,null,84,42,52,61,71,80,90,100,109,119,128]
[]
[]
[null,null,"Poundage per Gas Support in lbs. (2 Gas Supports per door)"]
[]
[null,null,null,"Width"]
[null,null,"Height",36,48,60,72,84,96,108,120,132,144]
[null,null,24]
[null,null,30]
[null,null,36]
[null,null,42]
[null,null,48]
[null,null,54]
[null,null,60]
[null,null,66,null,null,null,null,null,null,null,null,null,110]
[null,null,72,null,null,null,null,null,null,null,110,110,120]
[null,null,78,60,70,80,80,90,100,110,120,130,140]
[null,null,84,60,70,80,90,100,120,130,140,150,160]
[]
[null,null,null,null,"Placement \"A\" #5933 Gas Support",null,null,null,"Normal",null,"Stock Item"]
[null,null,null,null,"Placement \"B\" #5934 Gas Support",null,null,null,"Bold-Italic",null,"Non-Stock Item (Special Order)"]
[null,null,null,null,"Placement \"C\" #5934 Gas Support"]